**Mechanical sink mixer**

Single hole mechanical mixer with swivelling spout H. 220mm L. 200mm

Without pop-up waste

Reference: **2506T2**

Specification description

Deck-mounted mechanical sink mixer.

Single hole mechanical sink mixer with swivelling, tubular spout H. 220mm L. 200mm fitted with a hygienic flow straightener suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm ceramic cartridge with maximum temperature limiter supplied but not installed.

Spout with smooth interior.

Flow rate limited to 9 lpm at 3 bar.

Slimline control lever.

Without pop-up waste.

F3/8" PEX flexibles.

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.